PASS

## Summary

Report Date | 2025-06-26 05:12:36
Generated by | MemTest86 V11.3 Pro (64-bit)
Result | PASS

## System Information

EFI Specifications | 2.80
System |
Manufacturer | ADLINK Technology Inc.
Product Name | ADM-AL30
Version | Default string
Serial Number | Default string
BIOS |
Vendor | American Megatrends Inc.
Version | 0.08.11
Release Date | 05/27/2025
Baseboard |
Manufacturer | ADLINK Technology Inc.
Product Name | ADM-AL30
Version | A2
Serial Number | Default string
CPU Type | 12th Gen Intel Core i7-12700E
CPU Clock | 2134 MHz
# Logical Processors | 20 (12 enabled for testing)
L1 Cache | 32 x 80K (264666 MB/s)
L2 Cache | 8 x 1280K (56152 MB/s)
L3 Cache | 25600K (22470 MB/s)
Memory | 130789M (16554 MB/s)
RAM Configuration | DDR5 ECC 3590MT/s / x2 Channel / 30-29-29-57 / 1.100V
Number of RAM SPDs detected | 4
SPD #0 | 32GB DDR5 2Rx8 ECC PC5-38400
Vendor Part Info | InnoDisk Corporation / M5D0-BGS2Q5VP / 091D000A
JEDEC Profile | 4800MT/s 40-39-39-77 1.1V
SPD #1 | 32GB DDR5 2Rx8 ECC PC5-38400
Vendor Part Info | InnoDisk Corporation / M5D0-BGS2Q5VP / 091D000C
JEDEC Profile | 4800MT/s 40-39-39-77 1.1V
SPD #2 | 32GB DDR5 2Rx8 ECC PC5-38400
Vendor Part Info | InnoDisk Corporation / M5D0-BGS2Q5VP / 091D000B
JEDEC Profile | 4800MT/s 40-39-39-77 1.1V
SPD #3 | 32GB DDR5 2Rx8 ECC PC5-38400
Vendor Part Info | InnoDisk Corporation / M5D0-BGS2Q5VP / 091D000D
JEDEC Profile | 4800MT/s 40-39-39-77 1.1V
Number of RAM slots | 4
Number of RAM modules | 4
DIMM A1 | 32GB DDR5 2Rx8 ECC PC5-38400
Vendor Part Info | InnoDisk Corporation / M5D0-BGS2Q5VP / 091D000A
SMBIOS Profile | 4800MT/s 1.1V
DIMM A2 | 32GB DDR5 2Rx8 ECC PC5-38400
Vendor Part Info | InnoDisk Corporation / M5D0-BGS2Q5VP / 091D000C
SMBIOS Profile | 4800MT/s 1.1V
DIMM B1 | 32GB DDR5 2Rx8 ECC PC5-38400
Vendor Part Info | InnoDisk Corporation / M5D0-BGS2Q5VP / 091D000B
SMBIOS Profile | 4800MT/s 1.1V
DIMM B2 | 32GB DDR5 2Rx8 ECC PC5-38400
Vendor Part Info | InnoDisk Corporation / M5D0-BGS2Q5VP / 091D000D
SMBIOS Profile | 4800MT/s 1.1V

## Result summary

Test Start Time | 2025-06-26 02:13:44
Elapsed Time | 2:41:02
Memory Range Tested | 0x0 - 207F800000 (133112MB)
CPU Selection Mode | Parallel (All CPUs)
CPU Temperature Min/Max/Ave | 31C/42C/36C
RAM Temperature Min/Max/Ave |
TSOD0 | 33C/41C/37C
TSOD1 | 35C/46C/41C
TSOD2 | 32C/39C/36C
TSOD3 | 34C/44C/39C
Lowest memory speed | 3590 MT/s (30-29-29-57)
Highest memory speed | 3592 MT/s (30-29-29-57)
ECC Polling | Enabled
# Tests Completed | 14/14 (100%)
# Tests Passed | 14/14 (100%)

Test | # Tests Passed | Errors
Test 0 [Address test, walking ones, 1 CPU] | 1/1 (100%) | 0
Test 1 [Address test, own address, 1 CPU] | 1/1 (100%) | 0
Test 2 [Address test, own address] | 1/1 (100%) | 0
Test 3 [Moving inversions, ones & zeroes] | 1/1 (100%) | 0
Test 4 [Moving inversions, 8-bit pattern] | 1/1 (100%) | 0
Test 5 [Moving inversions, random pattern] | 1/1 (100%) | 0
Test 6 [Block move, 64-byte blocks] | 1/1 (100%) | 0
Test 7 [Moving inversions, 32-bit pattern] | 1/1 (100%) | 0
Test 8 [Random number sequence] | 1/1 (100%) | 0
Test 9 [Modulo 20, random pattern] | 1/1 (100%) | 0
Test 10 [Bit fade test, 2 patterns, 1 CPU] | 1/1 (100%) | 0
Test 11 [Random number sequence, 64-bit] | 1/1 (100%) | 0
Test 12 [Random number sequence, 128-bit] | 1/1 (100%) | 0
Test 13 [Hammer test] | 1/1 (100%) | 0